L1 IMS Mock Test Set 1

Section:

1

2

3

4

Time Left : 65 : 51 List View

Active Attempted Not Attempted

Q1

Before you attend a client call you should \_\_\_\_\_\_\_\_\_.

Multiple Choice - This may have multiple correct answers. Select required answer(s) from the options list.

Not care about the agenda of the call

Choose to display positive tone throughout the call

Practise what you will say and in which kind of pitch

Not care about the attendees

Q2

If your client speaks with a high rate of speech , you should \_\_\_\_\_\_\_\_\_\_\_\_\_\_. (choose all that applies)

Multiple Choice - This may have multiple correct answers. Select required answer(s) from the options list.

Stop listening

Make notes

Paraphrase / repeat the information in your own words

Ask questions for clarification

Q3

In an interview if a person has \_\_\_\_\_\_\_\_\_\_\_\_ thought process , he / she may not perform well.

Single Choice - Select one correct answer from the options list.

Innovative

Good

Limited

Satisfactory

None of the Above

Q4

You are angry and write an email in that mood, there is a possibility that \_\_\_\_\_\_\_\_\_\_\_\_\_. (choose all that applies)

Multiple Choice - This may have multiple correct answers. Select required answer(s) from the options list.

The tone of the email will not be affected at all

The words used will reflect your state of mind i.e. anger

The words used will reflect harmony & compassion

Tone will be negative

Q5

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ is an internal barrier to listening.

Single Choice - Select one correct answer from the options list.

Poor air conditioning in the room

The attitude of the speaker

Disinterestedness

Uncomfortable clothes worn

None of the Above

Q6

In almost all organizations most of the communication is done in the written form due to its many advantages like \_\_\_\_\_\_\_\_\_\_. ( Choose all that apply)

Multiple Choice - This may have multiple correct answers. Select required answer(s) from the options list.

It is inexpensive

Who has time to talk to others

It is a proof as is in a written form

It is beneficial for different time zones

Q7

Every employee or professional in an organization has Communication as his / her competency however the levels of proficiency may differ.

Single Choice - Select one correct answer from the options list.

FALSE

TRUE

Depends on factors

None of the above

Q8

Which statement is true?

Single Choice - Select one correct answer from the options list.

Listening is same as hearing

An external barrier to listening is prejudice

We must interrupt while listening

As compared to external barriers to listening , it takes time to overcome internal barriers.

None of the Above

Q9

While drafting an email in an office you should \_\_\_\_\_\_. (choose all that applies )

Multiple Choice - This may have multiple correct answers. Select required answer(s) from the options list.

Use complex words

Consider type of audience

Use simple English / easy language

Not consider the people in CC column

Q10

Which are the Do's of drafting a business email ? (choose all that apply)

Multiple Choice - This may have multiple correct answers. Select required answer(s) from the options list.

Avoid salutations in business emails

Proof read emails before sending

Always have a relevant subject line for your email

Create your own signature in business emails

Q11

Which of the following cron schedule will execute every weekday (i.e excluding Sat and Sun) during the working hours 9 a.m – 6 p.m?

Single Choice - Select one correct answer from the options list.

00 1-5 09-18 \* \* /home/ramesh/bin/check-db-status

00 \* 09-18 \* 1-5 /home/ramesh/bin/check-db-status

00 09-18 1-5 \* \* /home/ramesh/bin/check-db-status

00 09-18 1-5 \* \* /home/ramesh/bin/check-db-status

None of the Above

Q12

find and remove multiple files with the .mp3 extension?

Single Choice - Select one correct answer from the options list.

find . -type f -name "\*.mp3" -exec rm -f \;

find . -type f -name "\*.mp3" rm -f {} \;

find . -type f -name "\*.mp3" -exec rm {};

find . -type f -name "\*.mp3" -exec rm -f {} \;

None of the Above

Q13

Which of the following cron schedule will check the status of the database everyday (including weekends) during the working hours 9 a.m – 6 p.m?

Single Choice - Select one correct answer from the options list.

00 \* 09-18 \* \* \* /home/ramesh/bin/check-db-status

09-18 00 \* \* \* /home/ramesh/bin/check-db-status

00 \* \* \* 09-18 /home/ramesh/bin/check-db-status

00 \* \* 09-18 \* /home/ramesh/bin/check-db-status

None of the Above

Q14

Search in janes home folder for files ending with .doc and accessed in last 24 hours(or 1 day)

Single Choice - Select one correct answer from the options list.

find /home/jane/ -name \*.doc -time -1

**find /home/jane/ -name \*.doc -atime -1**

find /home/jane/ -name \*.doc -accessedtime -1

find /jane/ -name \*.doc -time -1

None of the Above

Q15

In useradd command, We need to use \_\_ switch to create the home directory if it didn't exist.

Single Choice - Select one correct answer from the options list.

m

c

**d**

p

None of the Above

Q16

Designed to offer support for Active Directory domain controllers running various supported operating systems by limiting functionality to specific software versions. As legacy domain controllers are decommissioned, administrators can modify the functional levels to expose new functionality within Active Directory. Some features in Active Directory cannot be activated, for example, until all domain controllers in a forest are upgraded to a specific level.

Single Choice - Select one correct answer from the options list.

external trust

container object

**functional levels**

directory service

None of the Above

Q17

\_\_\_\_ is a Special startup mode used to run an offline defragmentation.

Single Choice - Select one correct answer from the options list.

ADSM

DSMR

**DSRM**

DRSM

None of the Above

Q18

\_\_\_\_\_ is a Windows Server service that administrators can use to protect sensitive data on a Windows network.

Single Choice - Select one correct answer from the options list.

WINS

**RMS**

WDS

DFS

None of the Above

Q19

To Add execute permission for the owner and set the permissions for the group and others to read and execute, we need to use \_\_\_\_\_.

Single Choice - Select one correct answer from the options list.

**u+x, go=rx**

o+x, g=rx

go+x, o=rx

ugo=rx

None of the Above

Q20

\_\_\_\_ switch need to be used for listing all the system processes.

Single Choice - Select one correct answer from the options list.

**e**

a

s

l

None of the Above

Q21

Full name of an object that includes all hierarchical containers leading up to the root domain. The distinguished name begins with the object's common name and appends each succeeding parent container object, reflecting the object's location in the Active Directory structure.

Single Choice - Select one correct answer from the options list.

distinguished name (DN)

flat name

**Dns**

wds

None of the Above

Q22

\_\_\_\_ is used to define permission assignments. Administrators cannot manually modify the group membership.

Single Choice - Select one correct answer from the options list.

Global Group

Universal Group

Fixed Groups

**special identity group**

None of the Above

Q23

\_\_\_\_ is created whenever a new user is added to the system.

Single Choice - Select one correct answer from the options list.

UMG

**UPG**

UGM

UGP

None of the Above

Q24

First domain created within an Active Directory forest.

Single Choice - Select one correct answer from the options list.

**Domain Root**

Forest First

Forest Root

DC root

None of the Above

Q25

Which Flexible Single Master Operations (FSMO) role must be available in a domain to ensure that you are able to create accounts in that domain without any errors?

Single Choice - Select one correct answer from the options list.

**PDC Emulator**

RID Master

Schema Master

Domain Naming Master

None of the Above

Q26

\_\_\_\_\_\_ policy setting is appropriate for closely managed computers where the desktop configuration should remain the same, regardless of who logs on.

Single Choice - Select one correct answer from the options list.

Preference Targetting

WMI

Loopback Processing Mode

Item Level Targetting

None of the Above

Q27

What is the maximum number of subnets 174.19.22.14/25?

Single Choice - Select one correct answer from the options list.

128

**256**

512

1024

None of the Above

Q28

What is the need for "login" command?

Single Choice - Select one correct answer from the options list.

Used to set line password

Used to prompt the line password

this is used to log into the router

Used to Prompt all the passwords

None of the Above

Q29

\_\_\_\_\_\_ refers to the extra bits and characters added to data packets for error detection and control.

Single Choice - Select one correct answer from the options list.

**FCS**

CSMA

VTP

EMT

None of the Above

Q30

What is the broadcast address of 6.4.1.3/22?

Single Choice - Select one correct answer from the options list.

6.4.1.255

6.4.2.255

6.4.3.255

**6.4.255.255**

None of the Above

Q31

RARP is used for what purpose?

Single Choice - Select one correct answer from the options list.

**Map Source MAC To Source IP**

Map Destination IP to Destination MAC

MAP Source IP to Destination MAC

Map Destination IP to Source MAC

None of the Above

Q32

What is the port number used by SMTP?

Single Choice - Select one correct answer from the options list.

10

**25**

80

110

None of the Above

Q33

What is the total number of hosts in the network 172.16.64.0 / 21?

Single Choice - Select one correct answer from the options list.

11

**2 power 11 minus 2**

5

2 power 5 - 2

None of the Above

Q34

\_\_\_\_ command will remove a static route.

Single Choice - Select one correct answer from the options list.

remove ip route

rm ip route

**no ip route**

flush ip route

None of the Above

Q35

What is the last IP Address in the network 200.100.100.64/27?

Single Choice - Select one correct answer from the options list.

200.100.100.65

200.100.100.95

**200.100.100.94**

200.100.100.96

None of the Above

Q36

\_\_\_\_\_\_ command Encrypts the user mode and enable password.

Single Choice - Select one correct answer from the options list.

service encrypt

service password-encryption

**encrypt passwd**

password-encryption

None of the Above

Q37

For 120 Hosts what is the optimum subnet mask to be used in the VLSM Design?

Single Choice - Select one correct answer from the options list.

/24

**/25**

/26

/23

None of the Above

Q38

What is the Network address of 172.16.35.40 / 27?

Single Choice - Select one correct answer from the options list.

172.16.35.0

172.16.34.0

172.16.32.0

**172.16.35.32**

None of the Above

Q39

What is the maximum number of subnets that each subnet of 192.168.7.193/27 can accommodate?

Single Choice - Select one correct answer from the options list.

**30**

62

126

254

None of the Above

Q40

Is the IP Address 192.168.5.159 /28 valid?

Single Choice - Select one correct answer from the options list.

Yes

**No**

I don’t know

I don’t care

None of the Above

Q41

What is the Broadcast Address of the network 120.48.0.0/12?

Single Choice - Select one correct answer from the options list.

**120.48.255.255**

120.51.255.255

120.63.255.255

120.64.255.255

None of the Above

Q42

Is the IP Address 150.50.6.0 /22 valid?

Single Choice - Select one correct answer from the options list.

Yes

**No**

I don’t know

I don’t care

None of the Above

Q43

Which among these is not a network service?

Single Choice - Select one correct answer from the options list.

DHCP

DNS

BOOTP

**DBMS**

None of the Above

Q44

Which of the following is not a transmission medium?

Single Choice - Select one correct answer from the options list.

telephone lines

coaxial cables

**modem**

microwave systems

None of the Above

Q45

Expand LCN.

Single Choice - Select one correct answer from the options list.

**Left Cluster Number**

Live Cluster Number

LOCAL CLUSTER NUMBER

None of the Above

Q46

\_\_\_\_\_ is the filepath to the config params for GRUB.

Single Choice - Select one correct answer from the options list.

**/grub/grub.conf**

/etc/grub.conf

/grub.conf

/boot/grub.conf

None of the Above

Q47

Tables in second normal form (2NF):

Single Choice - Select one correct answer from the options list.

Eliminate all hidden dependencies

Eliminate the possibility of a insertion anomalies

Have a composite key

Have all non key fields depend on the whole primary key

None of the Above

Q48

Which is not the type of network?

Single Choice - Select one correct answer from the options list.

CAN

MAN

PAN

WAN

**None of the Above**

Q49

Which of these is not a DHCP message?

Single Choice - Select one correct answer from the options list.

DHCPLeasequery

DHCPLeaseunknown

DHCPLeaseunassigned

**DHCPLeaseabort**

None of the Above

Q50

\_\_\_\_\_ introduced the relational database rules.

Single Choice - Select one correct answer from the options list.

James Gosling

Dennies Rithchie

James Rambaugh

**None of the Above**

Q51

RS-232 is a standard that applies to?

Single Choice - Select one correct answer from the options list.

**serial ports**

parallel ports

game ports

networks

digital frequencies

None of the Above

Q52

Which of the following is NOT a type of motherboard expansion slot?

Single Choice - Select one correct answer from the options list.

ISA

PCI

AGP

**ATX**

None of the Above

Q53

Size of an MFT record?

Single Choice - Select one correct answer from the options list.

**1Kb**

2Kb

3Kb

4KB

None of the Above

Q54

Which of the following is NOT a type of RAM?

Single Choice - Select one correct answer from the options list.

DIMM

SIMM

**ROM**

SLIPP

None of the Above

Q55

Which of these is called Physical Memory?

Single Choice - Select one correct answer from the options list.

ROM

HDD

USB Disk

Page

**None of the Above**

Q56

NAS uses \_\_\_\_ IO.

Single Choice - Select one correct answer from the options list.

**Block**

File

Byte

Bit

None of the Above

Q57

NetBIOS stands for \_\_\_\_\_\_\_\_\_\_\_.

Single Choice - Select one correct answer from the options list.

Network BIOS Input/Output System

**Network Basic Input/Output System**

Networking Basic Input/Output System

Network Basic Input/Output Service

None of the Above

Q58

To copy a directory full of files in Linux, you must tell the cp command that the copy will be \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (involve files and subdirectories too) by using the \_\_\_\_ option.

Single Choice - Select one correct answer from the options list.

f

d

s

**R**

None of the Above

Q59

In a relational schema, each tuple is divided into fields called?

Single Choice - Select one correct answer from the options list.

**relations**

domains

queries

all the above

None of the Above

Q60

Parity is?

Single Choice - Select one correct answer from the options list.

a system for balancing the voltage coming out of the power supply

a byte stored in the FAT to indicated remaining slots

the last setting for controlling hard drive configuration of IDE drives in the CMOS

**an extra bit stored with data in RAM that is used to check for errors when the data is read back**

the optimal transmission speed of data over a CAT 5 cable

Q61

To create a hard link, you must use the \_\_\_\_ command.

Single Choice - Select one correct answer from the options list.

ls

lk

lh

**ln**

None of the Above

Q62

To create an encrypted password for use in the /boot/grub/grub.conf, you can use the \_\_\_\_ command.

Single Choice - Select one correct answer from the options list.

grub-md-crypt

grub-m5-crypt

**grub-md5-cryp**

None of the Above

Q63

IETF stands for \_\_\_\_\_\_\_\_\_\_\_\_\_\_.

Single Choice - Select one correct answer from the options list.

Internetwork Engineering Task Force

**Internet Engineering Task Force**

Internet Engineering Task Form

Internet Engineers Task Force

None of the Above

Q64

What is the sequence of data flow from physical layer to application layer?

Single Choice - Select one correct answer from the options list.

**Bits, Frames, Packet, Data**

Data, Packet, Bits

Bits, Packet, Frames, Data

None of the above

Q65

To see a list of all exported environment and user-defined variables in the shell, you can use the \_\_\_\_ command.

Single Choice - Select one correct answer from the options list.

**env**

exportall

exports

ex

None of the Above

Q66

A process enters the Blocked state when?

Single Choice - Select one correct answer from the options list.

**I/O Event**

Termination

Prempted

none

Q67

Foreign key is the one in which the \_\_\_\_\_\_\_\_ of one relation is referenced in another relation.

Single Choice - Select one correct answer from the options list.

Foreign key

**Primary key**

References

Check constraint

None of the Above

Q68

SOA stands for?

Single Choice - Select one correct answer from the options list.

**Service oriented architecture**

Simple oriented architecture

single object application

None of the above

Q69

Data will be in the form of \_\_\_\_\_\_\_\_, if it is fibre cable.

Single Choice - Select one correct answer from the options list.

packet

0’s

1’s

**light**

None of the Above

Q70

In the \_\_\_\_\_\_\_\_\_\_ normal form, a composite attribute is converted to individual attributes.

Single Choice - Select one correct answer from the options list.

**First**

Second

Third

Fourth

None of the Above

Q71

The most effective and effiecient topology is?

Single Choice - Select one correct answer from the options list.

Bus

**Star**

Ring

Mesh

None of the Above

Q72

Which of the following is not a valid RAID?

Single Choice - Select one correct answer from the options list.

10

01

4

**9**

None of the Above

Q73

What is the tool used to edit Group Policies locally?

Single Choice - Select one correct answer from the options list.

regedit.exe

services.msc

**gpedit.exe**

gpmc.msc

None of the Above

Q74

Updates that violate \_\_\_\_\_\_\_\_\_\_ are disallowed.

Single Choice - Select one correct answer from the options list.

**Integrity constraints**

Transaction control

Authorization

DDL constraints

None of the Above

Q75

What is framework?

Single Choice - Select one correct answer from the options list.

**Collection of libraries**

Collection of codes

Collection of program

collection of structured format

None of the Above

Business Communication

12345678910

IS Essentials 1

11121314151617181920212223242526

IS Essentials 2

27282930313233343536373839404142

IS Fundamentals

43444546474849505152535455565758596061626364656667686970717273747572 out of 75